Terminal / X/Y/Zmodem

This category only appears if VanDyke Software's SecureCRT® 5.0 (or newer) is also installed.

The Terminal/X/Y/Zmodem category of the Session Options dialog allows you to configure your Xmodem, Ymodem, and Zmodem settings.

Directories group

Upload

Enter the path of a local directory that is to be used as the source folder when the Upload command is used. Click on the browser button to select the directory.

Download

Enter the path of a local directory that is to be used as the destination folder when the Download command is used. Click on the browser button to select the directory.

X/Ymodem send packet size group

This group allows you to select the size of the Xmodem and Ymodem packets you send. Your options are as follows:

128 bytes

1024 bytes (Xmodem-1k/Ymodem-1k)

Zmodem

Disable Zmodem

Check this option to turn off the ability to make Zmodem transfers.

TFTP server group

Start TFTP server when session connects

Check this option to launch a TFTP server when the session connects. The TFTP server will use the upload and download directories specified in the Directories group in this category. Note that the upload and download directories are used opposite of how they are normally used in SecureCRT because the TFTP server is a server instead of a client.