Terminal / Advanced

This category only appears if VanDyke Software's SecureCRT® 5.0 (or newer) is also installed.

The Terminal/Advanced category of the Global Options dialog allows you to configure SecureCRT advanced terminal
A device usually consisting of a keyboard, a display unit such as a cathode ray tube,and a serial port used for entering and sending data to a computer and displaying any data received from the computer. Terminals are usually connected to a computer a serial line or some other type of connection. There are many terminal types including VT100, VT102, VT220, and others. emulation-related options.

Options group

This group contains various SecureCRT options.

Enable execute escape sequence

This option allows you to enable and disable the ability to send escape sequences.

Disable resize

Check this option to globally disallow the resizing of session
A session is a set of options that are assigned to a connection to a remote machine in SecureFX. These settings and options are saved under a session name and allow the user to have different preferences for different hosts. windows by means of the resize handles. Note that even though you may change the setting of this option globally, it is possible to make exceptions for one or more sessions by setting this option on a per session basis. Resizing the SecureCRT window can affect the number of rows and columns (see the Size group of the Session Options dialog, Terminal/Emulation category, for more information). By default, the Disable resize option is not selected.

Note: Full screen mode is not allowed when the Disable resize feature is set.

Connect to multiple sessions sequentially

When multiple sessions are connecting, check this option to have the sessions connect one after the other instead of all at once.

Disable session zooming with mouse scrollwheel

This option allows you to enable and disable the ability to use the mouse scrollwheel to zoom a session.

Swap ENTER and CTRL+ENTER in Command window

When this option is enabled, SecureCRT swaps the Command window behaviors of the ENTER key (send command, by default) and the CTRL+ENTER key combination (queue command, by default).

TFTP Server group

This group contains various SecureCRT options.

Listen port

Enter the UDP port on which the TFTP server will listen (default is 69).

Log file

Enter the location of the log file. If this option is left blank, SecureCRT will not save any log files.